# Foot PTT Protocol Format

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Header | Opcode | Length | Payload | Checksum | End |
| 1byte | 2bytes | 1byte | 1byte | 2bytes | 1byte |

Format description:

* Little-endian mode.
* Header: 0x7C.
* Opcode: 0xB001.
* Length: the length of payload.
* Payload:

0x01: Release PTT

0x00: Trigger PTT

* Checksum:

Checksum = Opcode + Length + Payload.

* End: 0x03.